The proxy offline browser archives visited web pages with your browser to be used on- and offline. Offline each page is available with its original URL. There is no difference between surfing in the internet or archive. You can even use your bookmarks offline. This proxy offline browser is an ideal addition to every browser!

Deutsch
| WebAssistant # Browser Proxy Configuration
| Private Professional
Switch on the proxy of your browser and enter the protocol types HTTP and FTP the IP address 127.0.0.1 and port 8080. # Settings for the browser Internet Explorer: Windows, Mac OS X Firefox Netscape and Mozilla Opera: Windows, Linux, Mac OS X Safari # Internet Explorer for Windows Please open a second window with the Internet Explorer (File/New/Window) at first. So you can do the settings and read this documentation simultaneously. Alternatively print this page, please.
## Menu bar (1) Select Tools (2) Select Internet Options.. |
## Dialog Internet Options (3) Select tab Connections ### ### Category Dial-up settings (4) Select Never dial a connection (5) Select used myDialUp item If you don't use a dial-up then go to point (15) LAN settings. (6) then click on Settings.. |
## Dialog myDialUp Settings ### Category Automatic configuration (7) Disable Automatically detect settings (8) Disable Use automatic configuration script ### Category Proxy server (9) Enable Use a proxy server for this connection (10) Disable Bypass proxy server for local addresses (11) and click on Advanced.. |
## Dialog Proxy Settings ### Category Servers (12) For the protocols HTTP and FTP enter the IP address 127.0.0.1 and port 8080. Note: If entries are already available here then you transfer these in the WebAssistant from Surf Sets/(HTTP-Protocol, FTP-Protocol). (13) Exit dialog Proxy Settings with OK. (14) Exit previous dialog myDialUp settings with OK. |
## Dialog Internet Options ### Category Local Area Network (LAN) settings (15) Click on LAN Settings.. |
## Dialog Local Area Network (Lan) Settings ### Category Automatic configuration (16) Disable Automatically detect settings (17) Disable Use automatic configuration script ### Category Proxy server (18) Enable Use a proxy server for your LAN (19) Disable Bypass proxy server for local addresses (20) and click on Advanced.. |
## Dialog Proxy Settings ### Category Servers (21) For the protocols HTTP and FTP enter the IP address 127.0.0.1 and port 8080. Note: If entries are already available here then you transfer these in the WebAssistant from Surf Sets/(HTTP-Protocol, FTP-Protocol). (22) Exit dialog Proxy Settings with OK. (23) Exit previous dialog Local Area Network (Lan) Settings with OK. |
## Dialog Internet Options (24) Select tab Advanced ### Category HTTP 1.1 settings (25) Enable Use HTTP 1.1 (26) Enable Use HTTP 1.1 through proxy connections (27) Exit dialog Internet Options with OK. |
Please, check now the installation with an offline- and an online-test.
| Installation |  | Installation test |
| © MM3Tools, 14-Dec-2005 | Legal information | WebAssistant@MM3Tools.com |